For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front floor console. Refer to Front Floor Console Replacement.
2. Remove the front floor console accessory housing. Refer to Front Floor Console Accessory Housing Replacement.
3. Remove the front floor console cover. Refer to Front Floor Rear Console Front Cover Replacement.

1 | Console Trim Plate Screws (Qty: 7) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Console Trim Plate