For 1990-2009 cars

## Front Side Marker Lamp Bulb Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse liner front in order to access the front side marker lamp bulb. Refer to Front Wheelhouse Front Liner Replacement.

1 | Front Side Marker Lamp Bulb Socket

#### Procedure

Rotate the bulb socket counter-clockwise and remove the socket from the park turn lamp housing.

2 | Front Side Marker Lamp Bulb Procedure Pull the marker lamp bulbs straight from the lamp bulb socket.

## Front Side Marker Lamp Bulb Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front wheelhouse liner in order to access the front turn signal bulbs. Refer to Front Wheelhouse Front Liner Replacement.
2. Disconnect the front marker lamp bulb socket from the headlamp assembly.

1 | Front Marker Lamp Bulb

#### Procedure

Pull the marker lamp bulbs straight from the lamp socket.

## Front Side Marker Lamp Bulb Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front wheelhouse liner in order to access the front turn signal bulbs. Refer to Front Wheelhouse Front Liner Replacement.
2. Disconnect the front marker lamp bulb socket from the headlamp assembly.

1 | Front Marker Lamp Bulb Cover

#### Procedure

Rotate the cover counterclockwise and remove the cover from the lamp housing.

2 | Front Marker Lamp Bulb

#### Procedure

Pull the marker lamp bulbs straight from the lamp socket.