For 1990-2009 cars

## Headlamp and Front End Fascia Mount Panel Replacement Base Acadia

Callout | Component Name
--- | ---

#### Procedure

Remove the headlamp assembly. Refer to Headlamp Replacement.

1 | Headlamp and Front Bumper Fascia Mounting Panel Support Screws (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten Tighten the screws to 2 N·m (18 lb in)
2 | Headlamp and Front Bumper Fascia Mounting Panel Support

## Headlamp and Front End Fascia Mount Panel Replacement HID Acadia

Callout | Component Name
--- | ---

#### Procedure

Remove the headlamp capsule. Refer to Headlamp Capsule Replacement.

1 | Headlamp and Front Bumper Fascia Mounting Panel Support Screws (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten Tighten the screws to 2 N·m (18 lb in)
2 | Headlamp and Front Bumper Fascia Mounting Panel Support

## Headlamp and Front End Fascia Mount Panel Replacement AFS Enclave

Callout | Component Name
--- | ---

#### Procedure

Remove the headlamp capsule. Refer to Headlamp Capsule Replacement.

1 | Headlamp and Front Bumper Fascia Mounting Panel Support Screws (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten Tighten the screws to 2 N·m (18 lb in)
2 | Headlamp and Front Bumper Fascia Mounting Panel Support

## Headlamp and Front End Fascia Mount Panel Replacement Base Enclave

Callout | Component Name
--- | ---

#### Procedure

Remove the headlamp assembly. Refer to Headlamp Replacement.

1 | Headlamp and Front Bumper Fascia Mounting Panel Support Screws (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten Tighten the screws to 2 N·m (18 lb in)
2 | Headlamp and Front Bumper Fascia Mounting Panel Support