For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Floor Console Rear Trim Cover Lower Panel Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rear Floor Console Rear Trim Lower Panel Assembly

#### Procedure

1. Disconnect the electrical connections.
2. When replacing the rear floor console rear trim lower panel assembly, transfer all necessary components.