For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Seat Adjuster Switch Mounting Plate

#### Procedure

1. Using a non-metallic flat-bladed tool, release the retainer tabs starting at the rear edge and working forward while pulling outward on the mounting plate.
2. Disconnect the electrical connectors from the switch assemblies.

2 | Front Seat Lumbar Control Switch Assembly Tip Use a flat-bladed tool to release the switch from the mounting plate.