For 1990-2009 cars

#### SIR Torque Specifications

Application | Specification
--- | ---
Metric | English
Airbag Attachment Bolt | 8 N·m | 71 lb in
Console Screws | 1.2 N·m | 11 lb in
Head Curtain Module Fastener | 8 N·m | 71 lb in
Inflator-to-Cross Car Beam | 8 N·m | 71 lb in
Passenger Inflator Module (Air Bag) Bolts | 10 N·m | 89 lb in
Passenger Inflator Module Cover Fasteners | 2.2 N·m | 20 lb in
Right I/P End Cap Fasteners | 2.2 N·m | 20 lb in
SDM Bolts | 10 N·m | 89 lb in
Side Airbag Tether Attachment Bolt | 8 N·m | 71 lb in
SIS Fasteners | 10 N·m | 89 lb in
Steering Column Shroud Fasteners | 4 N·m | 35 lb in
Steering Wheel Attachment Nut | 35 N·m | 26 lb ft
Upper Fill Tube Bolt | 2.5 N·m | 22 lb in
Upper I/P Trim Panel Fasteners | 6 N·m | 53 lb in