For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Door Stationary Glass (Sedan/Wagon) | 11 N·m | 97 lb in
Front Door Rear Window Guide Bolt | 6 N·m | 53 lb in
Front Window Regulator Bolts | 89 N·m | 10 lb in
Lower Quarter Trim Panel Fastener | 1.5 N·m | 13 lb in
Quarter Panel (Sedan) | 9 N·m | 80 lb in
Rear Side Door Stationary Window Fastener | 11 N·m | 97 lb in
Rear Window Regulator Bolts | 89 N·m | 10 lb in