For 1990-2009 cars

## Windshield Wiper Blade Replacement 1st Design

### Removal Procedure

Important: The right and left wiper blades are different lengths. Ensure that the longer blade is installed into the left-hand side.

1. Lift the wiper arm away from the glass.
2. Pinch the wiper blade attachment clip (1) together and slide the blade out of the wiper arm hook.

### Installation Procedure

1. Position the wiper arm blade into the wiper arm hook.
2. Slide the blade assembly into the hook until it clicks into position.

## Windshield Wiper Blade Replacement 2nd Design

### Removal Procedure

Important: The right and left wiper blades are different lengths. Ensure that the longer blade is installed into the left-hand side.

1. Lift the wiper arm away from the glass.
2. Pinch the wiper blade attachment clip (1) and slide the blade out of the wiper arm hook.

### Installation Procedure

1. Position the wiper arm blade into the wiper arm hook.
2. Slide the blade assembly into the hook until it clicks into position.