For 1990-2009 cars

### Removal Procedure

1. Remove the sunshade assembly from the sunroof. Refer to Sunroof Sunshade Replacement .
2. Squeeze together the fingers on the inboard end of the slide block to slide it out of its channel and remove the slide block and the spring.

### Installation Procedure

1. Insert the slide lock spring. Install the slide block by squeezing together the fingers on the inboard end of the slide block and inserting it into the sunshade.
2. Install the sunshade assembly. Refer to Sunroof Sunshade Replacement .